{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["BOM noms","BOM valeurs","Liste empreintes"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":4,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"BOM noms","index":0,"n_rows":116,"n_cols":12,"rows_kept":116,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Type","ID","Fonction","Valeur","Unité","Emprunte","Caractéristiques aditionnelles","Rem","Source","Code cmde","PU","OK"]
["Cap","C202","Alim","1µ","Farad",1206,"25V"]
["Cap","C203","Alim","100n","Farad",603]
["Cap","C206","Alim","1µ","Farad",1206,"25V"]
["Cap pol","C207","Alim","22µ","Farad","0606","35V"]
["Cap pol","C209","Alim","22µ","Farad","0606","35V"]
["Cap pol","C211","Alim","22µ","Farad","0606","35V"]
["Connect","J200","Alim",null,null,"SMT125-5","Alim 12V","5 points 2A nom"]
["Diode","D200","Alim",null,null,"LED0303","Led CMS","Led verte","Stock","-","-","X"]
["Diode","D204","Alim",null,null,"DO-214","S1G","anti inversion polarité"]
["Regu","U200","Alim",null,null,"TO252_5","TLE4275 5VLDO",null,"Stock","-","-","X"]
["Regu","U201","Alim",null,null,"TO252_5","TLE4276 LDO ajustable"]
["Regu","U202","Alim",null,null,"SOT-23","XC6206 LDO 2V5",null,"Farnell","?","?","X"]
["Res","R200","Alim","10K","Ohm",603,0.01,null,"Stock","-","-","X"]
["Res","R201","Alim","3K2","Ohm",603,0.01]
["Res","R202","Alim","10K","Ohm",603,0.01,null,"Stock","-","-","X"]
["Res","R208","Alim",470,"Ohm",603,null,null,"Stock","-","-","X"]
["Cap","C208","Alim","100n","Farad",603,"25V"]
["Cap","C801","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C802","FPGA","100n","Farad",603]
["Cap","C803","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C804","FPGA","100n","Farad",603]
["Cap","C805","FPGA","100n","Farad",603]
["Cap","C810","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C811","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C812","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C813","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C814","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C815","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C816","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C817","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C818","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C819","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C820","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C821","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C822","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C823","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C824","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C825","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C826","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C827","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C828","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C829","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C830","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C831","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C832","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C833","FPGA","10n","Farad",603,null,null,"Stock","-","-","X"]
["Cap","C843","FPGA","100n","Farad",603]
["Connect","JJTAG","FPGA",null,null,"PICOFL8","Emb Molex Picoflex 8pts","Connecteur JTAG","Farnell","865-527",null,"X"]
["Connect","JPS","FPGA",null,null,"PICOFL8","Emb Molex Picoflex 8pts","Connecteur passive serial","Farnell","865-527",null,"X"]
["FPGA","U800","FPGA",null,null,"TQFP-208",null,"ACEX EP1K50","Stock","-","-","X"]
["Mem","U802","FPGA",null,null,"PLCC20",null,"EPC2 : EEprom pour FPGA ALTERA","Stock","-","-","X"]
["Oscill","U801","FPGA","24M","Hz","OSC0705","CFPS-72 ","Oscillateur à quartz","Farnell","4245-982",7.11,"X"]
["Oscill","U803","FPGA","100M","Hz","OSC0503","CFPS-73","Oscillateur à quartz","Stock","-",0,"X"]
["Res","R800","FPGA",0,"Ohm",603,null,null,"Stock","-","-","X"]
["Res","R801","FPGA",100,"Ohm",603,null,null,"Stock","-","-","X"]
["Res","R802","FPGA",0,"Ohm",603,null,null,"Stock","-","-","X"]
["Res","R803","FPGA",100,"Ohm",603,null,null,"Stock","-","-","X"]
["Res","R804","FPGA","1K","Ohm",603,null,null,"Stock","-","-","X"]
["Res","R805","FPGA","1K","Ohm",603,null,null,"Stock","-","-","X"]
["Res","R806","FPGA","1K","Ohm",603,null,null,"Stock","-","-","X"]
["Res","R807","FPGA","1K","Ohm",603,null,null,"Stock","-","-","X"]
["Res","R808","FPGA","1K","Ohm",603,null,null,"Stock","-","-","X"]
["Res","R809","FPGA","1K","Ohm",603,null,null,"Stock","-","-","X"]
["Res","R810","FPGA",0,"Ohm",603,null,null,"Stock","-","-","X"]
["Res","R812","FPGA","1K","Ohm",603,null,null,"Stock","-","-","X"]
["Res","R813","FPGA","1K","Ohm",603,null,null,"Stock","-","-","X"]
["Res","R814","FPGA",47,"Ohm",603,null,null,"Stock","-","-","X"]
["Res","R816","FPGA",47,"Ohm",603,null,null,"Stock","-","-","X"]
["Res","R817","FPGA",47,"Ohm",603,null,null,"Stock","-","-","X"]
["Res","R818","FPGA",47,"Ohm",603,null,null,"Stock","-","-","X"]
["Res","R819","FPGA",47,"Ohm",603,null,null,"Stock","-","-","X"]
["Res","R820","FPGA",47,"Ohm",603,null,null,"Stock","-","-","X"]
["Res","R821","FPGA",47,"Ohm",603,null,null,"Stock","-","-","X"]
["Reseau R","RR1","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR2","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR3","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR4","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR5","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR7","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR8","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR9","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR10","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR11","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR12","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR13","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR14","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR15","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR16","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR17","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR18","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR19","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR22","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR23","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR24","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR25","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR26","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR27","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR28","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR29","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR30","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR31","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR32","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR33","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR34","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR35","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR36","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR37","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR38","FPGA",47,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Reseau R","RR39","FPGA",0,"Ohm","RR4X0603",null,null,"-","-","-","X"]
["Connect","JNORD","FPGA",null,null,"IDC56","HE10 2x28 pins 2,54mm","barette sécable","-","-","-","X"]
["Connect","JSUD","FPGA",null,null,"IDC56","HE10 2x28 pins 2,54mm","barette sécable","-","-","-","X"]
["Connect","JEST","FPGA",null,null,"IDC40","HE10 2x20 pins 2,54mm","barette sécable","-","-","-","X"]
["Connect","JOUEST","FPGA",null,null,"IDC40","HE10 2x20 pins 2,54mm","barette sécable","-","-","-","X"]
["Inter","S100","FPGA",null,null,"INVPCB","2x0603 tête bêche","1 seul res possible a la fois","-","-","-","X"]
["Inter","S101","FPGA",null,null,"INVPCB","2x0603 tête bêche","1 seul res possible a la fois","-","-","-","X"]

{"sheet":"BOM valeurs","index":1,"n_rows":28,"n_cols":11,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Type","Valeur","Unité","Emprunte","Caractéristiques aditionnelles","Rem","Qté","Source","Code cmde","PU","OK"]
["Cap","100n","Farad","0603",null,null,6]
["Cap","10n","Farad","0603",null,null,26]
["Cap","1µ","Farad","1206","25V","Céramique",2]
["Cap pol","22µ","Farad","0606","35V","ALU CMS",3]
["Connect",null,null,"PICOFL8","Emb Molex Picoflex 8pts","JTAG & passive serial",2,"Farnell","865-527",0.84,"X"]
["Connect",null,null,"IDC-40","2x20 points 2,54mm","barrette sécable HE10",2]
["Connect",null,null,"IDC-56","2x28 points 2,54mm","barrette sécable HE10",2]
["Connect",null,null,"SMT125-5","Connecteur alim","5 voies",1]
["Diode",null,null,"DO-214","S1G","Sur carte BM1005",1,"CARTES",null,null,"X"]
["Diode",null,null,"LED0303","LED CMS vertes","Alims + Prog_Done",1,"STOCK",null,null,"X"]
["FPGA",null,null,"TQFP-208","ACEX EP1K50","FPGA",1,"Stock",null,null,"X"]
["Osc","100M","Hz","OSC0503",null,"Oscillateur à quartz",1,"Stock","-",0,"X"]
["Osc","24M","Hz","OSC0705","CFPS-72 ","Oscillateur à quartz",1,"Farnell","424-5982",0,"X"]
["Régu",null,null,"TO252_5","TLE4275 5VLDO","Régu 5V",1,"Stock",null,null,"X"]
["Régu",null,null,"TO252_5","TLE4276 LDO ajustable","Régu 3V3 (ajustable)",1,"Stock",null,null,"X"]
["Régu",null,null,"SOT-23","XC6206 LDO 2V5","Régu 2V5",1,"Stock",null,null,"X"]
["Res",0,"Ohms","0603",0.05,null,3]
["Res",47,"Ohms","0603",0.05,null,7]
["Res",100,"Ohms","0603",0.05,null,2]
["Res",470,"Ohms","0603",0.05,null,1]
["Res","1K","Ohms","0603",0.05,null,8]
["Res","3,2K","Ohms","0603",0.01,null,1]
["Res","10K","Ohms","0603",0.01,null,2]
["Rés R",47,"Ohms","4X0603",0.05,null,35]
["Rés R",0,"Ohms","4X0603",0.05,null,1]
["Switch",0,"Ohms","InvPCB",null,"Switch de config à R 0603 0 Ohm",2]
["Mem",null,null,"PLCC20","EPC2LC20","EEPROM série 1Mo",1,"STOCK","-",0,"X"]

{"sheet":"Liste empreintes","index":2,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Emprunte","Caractéristiques aditionnelles","OK"]
["0606",null,null,null,"Fabriquée"]
["0603","0603 classique"]
["1206","1206 classique"]
["IDC-40","barrette HE10 2x20"]
["IDC-56","barrette HE10 2x28"]
["InvPCB","Switch 2 R 0603"]
["DO-214","S1G"]
["LED0303","LED CMS"]
["OSC0503","Oscillateur à quartz"]
["OSC0705","Oscillateur à quartz"]
["PLCC20","EEPROM FPGA"]
["SMT125-5","Connecteur Alim"]
["SOT-23","Régu 2V5"]
["TO252-5","Régu"]
["TQFP-208","FPgA"]
["PICOFL8","Emb Molex Picoflex 8pts"]
["4X0603","Réseau 4X0603"]